IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-01-22T10:52:50"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.0.0.383 - Exporter 21.0.0.383 - IU alternativa 21.0.0.383"
Application: "Autodesk Revit 2021 (ESP)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ESP)"

People and organizations
  Person "CYPE" of Organization (no name given)
  Owner history of Person "CYPE" of Organization (no name given) | application "Autodesk Revit 2021 (ESP)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ESP)" | change NOCHANGE | created 1610653881 (2021-01-14T19:51:21Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 59′ 27.599999″ | longitude -71° 27′ 39.599999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Manchester", "NH"
      IFCBUILDINGSTOREY "01 - Entry Level" | long name "01 - Entry Level" | object type "Nivel:8mm Head" | elevation 0.
        contains 267 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Superficie:105545" | names: "Superficie:105545"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Subregión:111931" | names: "Subregión:111931"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Superficie:130736" | names: "Superficie:130736"
          1 x IFCSITE | object type "Plataforma:Pad 1" | names: "Plataforma:Pad 1:130737"
          27 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Parking Space:5480 x 2740mm - 90 deg" | object type "M_Parking Space:5480 x 2740mm - 90 deg" | names: "M_Parking Space:5480 x 2740mm - 90 deg:130846", "M_Parking Space:5480 x 2740mm - 90 deg:130854", "M_Parking Space:5480 x 2740mm - 90 deg:132077" (+24 more) | material: "Parking Stripe" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters" | object type "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters" | names: "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters:134036", "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters:134052", "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters:134088" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Honey Locust - 7.6 Meters" | object type "M_RPC Tree - Deciduous:Honey Locust - 7.6 Meters" | names: "M_RPC Tree - Deciduous:Honey Locust - 7.6 Meters:134062", "M_RPC Tree - Deciduous:Honey Locust - 7.6 Meters:134064" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Shrub:Barberry - 1.0 Meters" | object type "M_RPC Shrub:Barberry - 1.0 Meters" | names: "M_RPC Shrub:Barberry - 1.0 Meters:135248", "M_RPC Shrub:Barberry - 1.0 Meters:135252", "M_RPC Shrub:Barberry - 1.0 Meters:135254" (+8 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Red Maple - 9 Meters" | object type "M_RPC Tree - Deciduous:Red Maple - 9 Meters" | names: "M_RPC Tree - Deciduous:Red Maple - 9 Meters:135276", "M_RPC Tree - Deciduous:Red Maple - 9 Meters:135284", "M_RPC Tree - Deciduous:Red Maple - 9 Meters:135286" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Golden Chain - 5.5 Meters" | object type "M_RPC Tree - Deciduous:Golden Chain - 5.5 Meters" | names: "M_RPC Tree - Deciduous:Golden Chain - 5.5 Meters:135328", "M_RPC Tree - Deciduous:Golden Chain - 5.5 Meters:135342" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Japanese Cherry - 4.5 Meters" | object type "M_RPC Tree - Deciduous:Japanese Cherry - 4.5 Meters" | names: "M_RPC Tree - Deciduous:Japanese Cherry - 4.5 Meters:135334", "M_RPC Tree - Deciduous:Japanese Cherry - 4.5 Meters:135336" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters" | object type "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters" | names: "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters:135386", "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters:135390", "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters:135392" (+3 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Exterior - Insulation on Masonry" | object type "Muro básico:Exterior - Insulation on Masonry" | names: "Muro básico:Exterior - Insulation on Masonry:139854", "Muro básico:Exterior - Insulation on Masonry:139857", "Muro básico:Exterior - Insulation on Masonry:144837" (+5 more) | material: layers "Muro básico:Exterior - Insulation on Masonry" ("Insulation / Thermal Barriers - External Wall Insulation" 100., "Masonry - Concrete Block" 190., "Plasterboard" 13.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          16 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Exterior Curtain Wall" | object type "Muro cortina:Exterior Curtain Wall" | names: "Muro cortina:Exterior Curtain Wall:139855", "Muro cortina:Exterior Curtain Wall:139856", "Muro cortina:Exterior Curtain Wall:139858" (+13 more) | parts: 2392 IFCMEMBER, 1023 IFCPLATE, 4 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Pavillion Curtain Wall" | object type "Muro cortina:Pavillion Curtain Wall" | names: "Muro cortina:Pavillion Curtain Wall:140012", "Muro cortina:Pavillion Curtain Wall:140015", "Muro cortina:Pavillion Curtain Wall:140018" | parts: 346 IFCMEMBER, 145 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          53 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:140949", "M_Concrete-Round-Column:300mm:140950", "M_Concrete-Round-Column:300mm:140951" (+50 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:140988" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:140992" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          32 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):143858", "Muro básico:Interior - 138mm Partition (1-hr):144051", "Muro básico:Interior - 138mm Partition (1-hr):144180" (+29 more) | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Generic - 200mm" | object type "Muro básico:Generic - 200mm" | names: "Muro básico:Generic - 200mm:144344", "Muro básico:Generic - 200mm:150861", "Muro básico:Generic - 200mm:151331" (+1 more) | material: layers "Muro básico:Generic - 200mm" ("Default Wall" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):145023" | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1220mm" | object type "M_Fixed:0915 x 1220mm" | names: "M_Fixed:0915 x 1220mm:145607", "M_Fixed:0915 x 1220mm:145683", "M_Fixed:0915 x 1220mm:145733" (+3 more) | material: materials ("Glass", "Sash") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush-Dbl Acting:0915 x 2134mm" | object type "M_Single-Flush-Dbl Acting:0915 x 2134mm" | names: "M_Single-Flush-Dbl Acting:0915 x 2134mm:145999" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          9 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:146094", "M_Single-Flush:0915 x 2134mm:146343", "M_Single-Flush:0915 x 2134mm:146563" (+6 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | object type "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | names: "M_Single-Flush:0915 x 2134mm 20 Minute Rated:146152", "M_Single-Flush:0915 x 2134mm 20 Minute Rated:152476" | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1830 x 2134mm" | object type "M_Double-Flush:1830 x 2134mm" | names: "M_Double-Flush:1830 x 2134mm:146282" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          10 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:146483", "M_Single-Flush:0915 x 2134mm:146641", "M_Single-Flush:0915 x 2134mm:150403" (+7 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:146741" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:147476" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:147486" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:147494" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:147502" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Plain" | object type "Techo compuesto:Plain" | CEILING | names: "Techo compuesto:Plain:147510" | material: layers "Techo compuesto:Plain" ("Metal - Stud Layer" 45., "Plasterboard" 12.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Plain" | object type "Techo compuesto:Plain" | CEILING | names: "Techo compuesto:Plain:147518" | material: layers "Techo compuesto:Plain" ("Metal - Stud Layer" 45., "Plasterboard" 12.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:147534" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Storefront" | object type "Muro cortina:Storefront" | names: "Muro cortina:Storefront:147833", "Muro cortina:Storefront:148960", "Muro cortina:Storefront:151588" (+1 more) | parts: 122 IFCMEMBER, 39 IFCPLATE, 4 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm" | object type "M_Double-Flush:1730 x 2134mm" | names: "M_Double-Flush:1730 x 2134mm:149921" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | object type "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | names: "M_Double-Flush:1730 x 2134mm 20 Minute Rated:150034" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | object type "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | names: "M_Double-Flush:1730 x 2134mm 20 Minute Rated:150153" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1830 x 2134mm" | object type "M_Double-Flush:1830 x 2134mm" | names: "M_Double-Flush:1830 x 2134mm:150584" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:155278" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Generic - 225mm Concrete" | object type "Muro básico:Generic - 225mm Concrete" | names: "Muro básico:Generic - 225mm Concrete:155851", "Muro básico:Generic - 225mm Concrete:155993", "Muro básico:Generic - 225mm Concrete:156072" (+1 more) | material: layers "Muro básico:Generic - 225mm Concrete" ("Concrete - Cast-in-Place Concrete" 225.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Standard Timber-Wood Finish" | object type "Suelo:Standard Timber-Wood Finish" | FLOOR | names: "Suelo:Standard Timber-Wood Finish:156686" | material: layers "Suelo:Standard Timber-Wood Finish" ("Wood - Flooring" 40., "Concrete - Cast-in-Place Concrete" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168641" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168649" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168657" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168671" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168679" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168687" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168695" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168703" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168711" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168719" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168727" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168735" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          5 x IFCSTAIR | object type "Escalera:150mm max riser 300mm tread" | names: "Escalera:150mm max riser 300mm tread:172987", "Escalera:150mm max riser 300mm tread:173290", "Escalera:150mm max riser 300mm tread:180746" (+2 more) | parts: 16 IFCMEMBER, 13 IFCRAILING, 10 IFCSTAIRFLIGHT, 5 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201146" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201155" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201164" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201173" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201271" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201272" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201273" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201274" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201275" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | object type "M_W-Wide Flange-Column:W250X49.1" | names: "M_W-Wide Flange-Column:W250X49.1:201276" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:450mm" | object type "M_Concrete-Round-Column:450mm" | names: "M_Concrete-Round-Column:450mm:201277", "M_Concrete-Round-Column:450mm:201278", "M_Concrete-Round-Column:450mm:201279" (+3 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Concrete- 100mm" | object type "Suelo:Concrete- 100mm" | FLOOR | names: "Suelo:Concrete- 100mm:212675" | material: layers "Suelo:Concrete- 100mm" ("Concrete - Cast-in-Place Concrete" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Borde de losa:Slab Edge" | object type "Borde de losa:Slab Edge" | names: "Borde de losa:Slab Edge:217842" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Borde de losa:Slab Edge" | object type "Borde de losa:Slab Edge" | names: "Borde de losa:Slab Edge:217846" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "101" | long name "Vest." | INTERNAL
        IFCSPACE "102" | long name "Lobby" | INTERNAL
        IFCSPACE "103" | long name "Conference" | INTERNAL
        IFCSPACE "104" | long name "Instruction" | INTERNAL
        IFCSPACE "105" | long name "Instruction" | INTERNAL
        IFCSPACE "106" | long name "Instruction" | INTERNAL
        IFCSPACE "107" | long name "Corridor" | INTERNAL
        IFCSPACE "108" | long name "Instruction" | INTERNAL
        IFCSPACE "109" | long name "Women" | INTERNAL
        IFCSPACE "110" | long name "Men" | INTERNAL
        IFCSPACE "111" | long name "Lounge" | INTERNAL
        IFCSPACE "112" | long name "Electrical" | INTERNAL
        IFCSPACE "114" | long name "Stair" | INTERNAL
        IFCSPACE "115" | long name "Instruction" | INTERNAL
        IFCSPACE "116" | long name "Conference" | INTERNAL
        IFCSPACE "117" | long name "Instruction" | INTERNAL
        IFCSPACE "118" | long name "Electrical" | INTERNAL
        IFCSPACE "119" | long name "Sprinkler" | INTERNAL
        IFCSPACE "120" | long name "Lounge" | INTERNAL
        IFCSPACE "121" | long name "Cafeteria" | INTERNAL
          contains 75 elements
            15 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "M_Table-Dining Round w Chairs:0915mm Diameter" | object type "M_Table-Dining Round w Chairs:0915mm Diameter" | names: "M_Table-Dining Round w Chairs:0915mm Diameter:180294", "M_Table-Dining Round w Chairs:0915mm Diameter:180360", "M_Table-Dining Round w Chairs:0915mm Diameter:180416" (+12 more) | material: materials ("Wood - Pine", "Laminate - Linen, Matte") | property sets: Pset_QuantityTakeOff
            60 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "M_Chair-Breuer:M_Chair-Breuer" | object type "M_Chair-Breuer:M_Chair-Breuer" | names: "M_Chair-Breuer:M_Chair-Breuer:180296", "M_Chair-Breuer:M_Chair-Breuer:180297", "M_Chair-Breuer:M_Chair-Breuer:180298" (+57 more) | material: materials ("Textile - Bamboo Weave", "Metal - Chrome") | property sets: Pset_QuantityTakeOff
        IFCSPACE "122" | long name "Prep/Dish" | INTERNAL
        IFCSPACE "123" | long name "Conference" | INTERNAL
        IFCSPACE "124" | long name "Dry Storage" | INTERNAL
        IFCSPACE "125" | long name "Electrical" | INTERNAL
        IFCSPACE "126" | long name "Admin" | INTERNAL
        IFCSPACE "127" | long name "Office" | INTERNAL
        IFCSPACE "128" | long name "Storage" | INTERNAL
        IFCSPACE "129" | long name "Toilet" | INTERNAL
        IFCSPACE "130" | long name "Stair" | INTERNAL
        IFCSPACE "131" | long name "Corridor" | INTERNAL
        IFCSPACE "132" | long name "Stair" | INTERNAL
        IFCSPACE "1" | long name "Service" | INTERNAL
        IFCSPACE "2" | long name "Administration" | INTERNAL
        IFCSPACE "3" | long name "Cirrculation" | INTERNAL
        IFCSPACE "4" | long name "Service" | INTERNAL
        IFCSPACE "5" | long name "Service" | INTERNAL
        IFCSPACE "6" | long name "Instruction" | INTERNAL
        IFCSPACE "7" | long name "Service" | INTERNAL
        IFCSPACE "8" | long name "Instruction" | INTERNAL
        IFCSPACE "9" | long name "Service" | INTERNAL
      IFCBUILDINGSTOREY "02 - Floor" | long name "02 - Floor" | object type "Nivel:8mm Head" | elevation 3800.00000000151
        contains 185 elements
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Hollow Core Plank - Concrete Topping" | object type "Suelo:Hollow Core Plank - Concrete Topping" | FLOOR | names: "Suelo:Hollow Core Plank - Concrete Topping:139803" | material: layers "Suelo:Hollow Core Plank - Concrete Topping" ("Carpet (1)" 15., "Concrete - Cast-in-Place Concrete" 50., "Concrete - Cast In Situ" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          54 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141184", "M_Concrete-Round-Column:300mm:141185", "M_Concrete-Round-Column:300mm:141186" (+51 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          44 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):157640", "Muro básico:Interior - 138mm Partition (1-hr):157641", "Muro básico:Interior - 138mm Partition (1-hr):157642" (+41 more) | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          11 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:157648", "M_Single-Flush:0915 x 2134mm:157696", "M_Single-Flush:0915 x 2134mm:157700" (+8 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          6 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Storefront" | object type "Muro cortina:Storefront" | names: "Muro cortina:Storefront:157650", "Muro cortina:Storefront:157669", "Muro cortina:Storefront:157673" (+3 more) | parts: 159 IFCMEMBER, 52 IFCPLATE, 5 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):157695" | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | object type "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | names: "M_Single-Flush:0915 x 2134mm 20 Minute Rated:157697" | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          12 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:157699", "M_Single-Flush:0915 x 2134mm:158537", "M_Single-Flush:0915 x 2134mm:158647" (+9 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | object type "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | names: "M_Single-Flush:0915 x 2134mm 20 Minute Rated:159676" | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | object type "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | names: "M_Double-Flush:1730 x 2134mm 20 Minute Rated:161727" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168750" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168758" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168766" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168774" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168782" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168790" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168798" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168806" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168832" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168846" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168854" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168868" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168878" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168886" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168894" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168902" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168910" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168918" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168926" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168934" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168942" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168950" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168958" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168966" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Exterior Curtain Wall" | object type "Muro cortina:Exterior Curtain Wall" | names: "Muro cortina:Exterior Curtain Wall:169402", "Muro cortina:Exterior Curtain Wall:169602" | parts: 68 IFCMEMBER, 24 IFCPLATE | property sets: Pset_OpeningElementCommon, Pset_QuantityTakeOff
          5 x IFCSTAIR | object type "Escalera:150mm max riser 300mm tread" | names: "Escalera:150mm max riser 300mm tread:172987", "Escalera:150mm max riser 300mm tread:173290", "Escalera:150mm max riser 300mm tread:180746" (+2 more) | parts: 16 IFCMEMBER, 13 IFCRAILING, 10 IFCSTAIRFLIGHT, 5 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          9 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1220mm" | object type "M_Fixed:0915 x 1220mm" | names: "M_Fixed:0915 x 1220mm:198996", "M_Fixed:0915 x 1220mm:199047", "M_Fixed:0915 x 1220mm:199097" (+6 more) | material: materials ("Glass", "Sash") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201191" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201200" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201209" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201218" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCROOF | object type "Cubierta básica:Generic - 75mm" | names: "Cubierta básica:Generic - 75mm:201262" | parts: 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | object type "Techo compuesto:Furred Ceiling" | CEILING | names: "Techo compuesto:Furred Ceiling:247617" | material: layers "Techo compuesto:Furred Ceiling" ("Metal - Stud Layer" 22.2, "Plasterboard" 15.9) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | object type "Techo compuesto:Furred Ceiling" | CEILING | names: "Techo compuesto:Furred Ceiling:247677" | material: layers "Techo compuesto:Furred Ceiling" ("Metal - Stud Layer" 22.2, "Plasterboard" 15.9) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          6 x IFCRAILING | object type "Barandilla:Guardrail - Pipe" | names: "Barandilla:Guardrail - Pipe:176909", "Barandilla:Guardrail - Pipe:234986", "Barandilla:Guardrail - Pipe:235001" (+3 more) | material: "Metal - Bronze" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
        IFCSPACE "201" | long name "Stair" | INTERNAL
        IFCSPACE "202" | long name "Instruction" | INTERNAL
        IFCSPACE "203" | long name "Computer Lab" | INTERNAL
        IFCSPACE "204" | long name "Instruction" | INTERNAL
        IFCSPACE "205" | long name "Instruction" | INTERNAL
        IFCSPACE "206" | long name "Lounge" | INTERNAL
        IFCSPACE "207" | long name "Copy/Print" | INTERNAL
        IFCSPACE "208" | long name "Drafting" | INTERNAL
        IFCSPACE "209" | long name "Computer Lab" | INTERNAL
        IFCSPACE "210" | long name "Men" | INTERNAL
        IFCSPACE "211" | long name "Women" | INTERNAL
        IFCSPACE "212" | long name "Lounge" | INTERNAL
        IFCSPACE "214" | long name "Electrical" | INTERNAL
        IFCSPACE "216" | long name "Lobby" | INTERNAL
          contains 14 elements
            14 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pendant Light - Linear - 1 Lamp:2440mm - 277V" | object type "Pendant Light - Linear - 1 Lamp:2440mm - 277V" | names: "Pendant Light - Linear - 1 Lamp:2440mm - 277V:247920", "Pendant Light - Linear - 1 Lamp:2440mm - 277V:247921", "Pendant Light - Linear - 1 Lamp:2440mm - 277V:248028" (+11 more) | material: materials ("Glass - White, High Luminance", "Paint - Maroon Glossy", "Metal - Paint Finish - Ivory, Glossy", "Default Light Source") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
        IFCSPACE "217" | long name "Stair" | INTERNAL
        IFCSPACE "218" | long name "Instruction" | INTERNAL
        IFCSPACE "219" | long name "Library" | INTERNAL
        IFCSPACE "220" | long name "Electrical" | INTERNAL
        IFCSPACE "221" | long name "Instruction" | INTERNAL
        IFCSPACE "222" | long name "Computer Lab" | INTERNAL
        IFCSPACE "223" | long name "Lounge" | INTERNAL
        IFCSPACE "224" | long name "Caferteria" | INTERNAL
        IFCSPACE "225" | long name "Women" | INTERNAL
        IFCSPACE "226" | long name "Men" | INTERNAL
        IFCSPACE "227" | long name "Electrical" | INTERNAL
        IFCSPACE "228" | long name "Copy/Print" | INTERNAL
        IFCSPACE "229" | long name "Administration" | INTERNAL
        IFCSPACE "230" | long name "Office" | INTERNAL
        IFCSPACE "231" | long name "Office" | INTERNAL
        IFCSPACE "232" | long name "Toilet" | INTERNAL
        IFCSPACE "233" | long name "Stair" | INTERNAL
        IFCSPACE "234" | long name "Corridor" | INTERNAL
        IFCSPACE "235" | long name "Corridor" | INTERNAL
        IFCSPACE "10" | long name "Cirrculation" | INTERNAL
        IFCSPACE "11" | long name "Service" | INTERNAL
        IFCSPACE "12" | long name "Administration" | INTERNAL
        IFCSPACE "13" | long name "Service" | INTERNAL
        IFCSPACE "14" | long name "Instruction" | INTERNAL
        IFCSPACE "15" | long name "Service" | INTERNAL
        IFCSPACE "16" | long name "Instruction" | INTERNAL
        IFCSPACE "17" | long name "Instruction" | INTERNAL
        IFCSPACE "18" | long name "Service" | INTERNAL
      IFCBUILDINGSTOREY "03 - Floor" | long name "03 - Floor" | object type "Nivel:8mm Head" | elevation 7599.99999999994
        contains 172 elements
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Hollow Core Plank - Concrete Topping" | object type "Suelo:Hollow Core Plank - Concrete Topping" | FLOOR | names: "Suelo:Hollow Core Plank - Concrete Topping:139829" | material: layers "Suelo:Hollow Core Plank - Concrete Topping" ("Carpet (1)" 15., "Concrete - Cast-in-Place Concrete" 50., "Concrete - Cast In Situ" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141254" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141255" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141256" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141257" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141258" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141259" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141260" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141261" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141262" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141263" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141265" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141266" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141267" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141268" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141269" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141270" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141271" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141272" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141276" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141277" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141278" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141279" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141280" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141281" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141282" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141283" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141284" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141285" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141286" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141287" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141288" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141290" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141291" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141293" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141294" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141295" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141296" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141299" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141300" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141301" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141302" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141303" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141304" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141305" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141306" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141309" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141310" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141311" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141312" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141313" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141314" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141315" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141316" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141317" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | object type "M_Concrete-Round-Column:300mm" | names: "M_Concrete-Round-Column:300mm:141318" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCROOF | object type "Cubierta básica:Generic - 400mm" | names: "Cubierta básica:Generic - 400mm:142430" | parts: 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          31 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):157778", "Muro básico:Interior - 138mm Partition (1-hr):157779", "Muro básico:Interior - 138mm Partition (1-hr):157780" (+28 more) | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:157786", "M_Single-Flush:0915 x 2134mm:157834", "M_Single-Flush:0915 x 2134mm:157838" (+6 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Storefront" | object type "Muro cortina:Storefront" | names: "Muro cortina:Storefront:157788", "Muro cortina:Storefront:157811", "Muro cortina:Storefront:157854" | parts: 69 IFCMEMBER, 24 IFCPLATE, 3 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):157833" | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | object type "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | names: "M_Single-Flush:0915 x 2134mm 20 Minute Rated:157835" | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          10 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:157837", "M_Single-Flush:0915 x 2134mm:163587", "M_Single-Flush:0915 x 2134mm:163637" (+7 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush Vision:0915 x 2134mm" | object type "M_Single-Flush Vision:0915 x 2134mm" | names: "M_Single-Flush Vision:0915 x 2134mm:164566", "M_Single-Flush Vision:0915 x 2134mm:164768" | material: materials ("Paint - Maroon Glossy", "Glass", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush Vision:0915 x 2134mm" | object type "M_Single-Flush Vision:0915 x 2134mm" | names: "M_Single-Flush Vision:0915 x 2134mm:164626", "M_Single-Flush Vision:0915 x 2134mm:164869" | material: materials ("Paint - Maroon Glossy", "Glass", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | object type "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | names: "M_Single-Flush:0915 x 2134mm 20 Minute Rated:164674" | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Glass 1:1830 x 2134mm" | object type "M_Double-Glass 1:1830 x 2134mm" | names: "M_Double-Glass 1:1830 x 2134mm:165368" | material: materials ("Paint - Maroon Glossy", "Glass", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | object type "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | names: "M_Double-Flush:1730 x 2134mm 20 Minute Rated:165462" | material: materials ("Door - Panel", "Door - Frame") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Glass 1:0915 x 2134mm" | object type "M_Single-Glass 1:0915 x 2134mm" | names: "M_Single-Glass 1:0915 x 2134mm:165525" | material: materials ("Paint - Maroon Glossy", "Glass", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168986" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:168996" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169004" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169012" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169026" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169040" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169048" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169056" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169064" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169072" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169082" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169090" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169098" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169106" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169114" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169122" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169130" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169138" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | object type "Techo compuesto:600 x 600mm Grid" | CEILING | names: "Techo compuesto:600 x 600mm Grid:169146" | material: layers "Techo compuesto:600 x 600mm Grid" ("Default" 36., "Ceiling Tile 600 x 600" 16.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          9 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1220mm" | object type "M_Fixed:0915 x 1220mm" | names: "M_Fixed:0915 x 1220mm:199360", "M_Fixed:0915 x 1220mm:199402", "M_Fixed:0915 x 1220mm:199436" (+6 more) | material: materials ("Glass", "Sash") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:200929" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201054" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201078" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Metal Sunscreen" | object type "Suelo:Metal Sunscreen" | FLOOR | names: "Suelo:Metal Sunscreen:201128" | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | object type "Techo compuesto:Furred Ceiling" | CEILING | names: "Techo compuesto:Furred Ceiling:242937" | material: layers "Techo compuesto:Furred Ceiling" ("Metal - Stud Layer" 22.2, "Plasterboard" 15.9) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          16 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pendant Light - Linear - 1 Lamp:2440mm - 277V" | object type "Pendant Light - Linear - 1 Lamp:2440mm - 277V" | names: "Pendant Light - Linear - 1 Lamp:2440mm - 277V:243204", "Pendant Light - Linear - 1 Lamp:2440mm - 277V:243343", "Pendant Light - Linear - 1 Lamp:2440mm - 277V:243410" (+13 more) | material: materials ("Glass - White, High Luminance", "Paint - Maroon Glossy", "Metal - Paint Finish - Ivory, Glossy", "Default Light Source") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCRAILING | object type "Barandilla:Guardrail - Pipe" | names: "Barandilla:Guardrail - Pipe:234238", "Barandilla:Guardrail - Pipe:234889", "Barandilla:Guardrail - Pipe:234946" | material: "Metal - Bronze" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
        IFCSPACE "301" | long name "Stair" | INTERNAL
        IFCSPACE "302" | long name "Instruction" | INTERNAL
        IFCSPACE "303" | long name "Instruction" | INTERNAL
        IFCSPACE "304" | long name "Instruction" | INTERNAL
        IFCSPACE "305" | long name "Instruction" | INTERNAL
        IFCSPACE "306" | long name "Instruction" | INTERNAL
        IFCSPACE "307" | long name "Men" | INTERNAL
        IFCSPACE "308" | long name "Women" | INTERNAL
        IFCSPACE "309" | long name "Lounge" | INTERNAL
        IFCSPACE "310" | long name "Electrical" | INTERNAL
        IFCSPACE "312" | long name "Stair" | INTERNAL
        IFCSPACE "313" | long name "Instruction" | INTERNAL
        IFCSPACE "314" | long name "Instruction" | INTERNAL
        IFCSPACE "315" | long name "Instruction" | INTERNAL
        IFCSPACE "316" | long name "Storage" | INTERNAL
        IFCSPACE "317" | long name "Electrical" | INTERNAL
        IFCSPACE "318" | long name "Lobby" | INTERNAL
          contains 45 elements
            7 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Chair-Viper:Chair" | object type "Chair-Viper:Chair" | names: "Chair-Viper:Chair:235333", "Chair-Viper:Chair:235334", "Chair-Viper:Chair:235335" (+4 more) | material: materials ("Leather - Brown, Pebble", "Chrome") | property sets: Pset_QuantityTakeOff
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Couch-Viper:Couch" | object type "Couch-Viper:Couch" | names: "Couch-Viper:Couch:235336", "Couch-Viper:Couch:235337", "Couch-Viper:Couch:235342" | material: materials ("Leather - Tan", "Metal - Chrome") | property sets: Pset_QuantityTakeOff
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Wastebasket2:Wastebasket2" | object type "Wastebasket2:Wastebasket2" | names: "Wastebasket2:Wastebasket2:235343", "Wastebasket2:Wastebasket2:235344", "Wastebasket2:Wastebasket2:235345" (+1 more) | material: "Plastic - Dark Maroon, Smooth" | property sets: Pset_QuantityTakeOff
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Table-Night Stand:24" x 24" x 30"" | object type "Table-Night Stand:24" x 24" x 30"" | names: "Table-Night Stand:24" x 24" x 30":235347", "Table-Night Stand:24" x 24" x 30":235348", "Table-Night Stand:24" x 24" x 30":235349" (+6 more) | material: "Wood - Cherry" | property sets: Pset_QuantityTakeOff
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Potted Plant:Potted Plant" | object type "Potted Plant:Potted Plant" | names: "Potted Plant:Potted Plant:235355", "Potted Plant:Potted Plant:235356" | material: "Ceramic - Tan" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            4 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Table Lamp 4:60 watt Incandescent" | object type "Table Lamp 4:60 watt Incandescent" | names: "Table Lamp 4:60 watt Incandescent:235371", "Table Lamp 4:60 watt Incandescent:235372", "Table Lamp 4:60 watt Incandescent:235373" (+1 more) | material: materials ("Metal - Bronze", "Shade - Beige, texture", "Default Light Source") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
            7 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Sconce 4:40 watt Halogen" | object type "Sconce 4:40 watt Halogen" | names: "Sconce 4:40 watt Halogen:245151", "Sconce 4:40 watt Halogen:245907", "Sconce 4:40 watt Halogen:245958" (+4 more) | material: materials ("Default Light Source", "Glass - Clear Light", "Metal - Chrome") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:246168" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:247101" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:247145" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:247176" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:247241" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Window Shade:Window Shade" | object type "Window Shade:Window Shade" | names: "Window Shade:Window Shade:247523" | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Male:Alex" | object type "M_RPC Male:Alex" | names: "M_RPC Male:Alex:248914" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Male:Jay" | object type "M_RPC Male:Jay" | names: "M_RPC Male:Jay:248959" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_RPC Female:Florence" | object type "M_RPC Female:Florence" | names: "M_RPC Female:Florence:249454" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
        IFCSPACE "319" | long name "Media Review" | INTERNAL
        IFCSPACE "320" | long name "Media Review" | INTERNAL
        IFCSPACE "321" | long name "Open Office" | INTERNAL
        IFCSPACE "322" | long name "Administration" | INTERNAL
        IFCSPACE "323" | long name "Electrical" | INTERNAL
        IFCSPACE "324" | long name "Advisors" | INTERNAL
        IFCSPACE "325" | long name "Conference" | INTERNAL
        IFCSPACE "326" | long name "Toilet" | INTERNAL
        IFCSPACE "327" | long name "Stair" | INTERNAL
        IFCSPACE "328" | long name "Corridor" | INTERNAL
        IFCSPACE "19" | long name "Cirrculation" | INTERNAL
        IFCSPACE "20" | long name "Instruction" | INTERNAL
        IFCSPACE "21" | long name "Service" | INTERNAL
        IFCSPACE "22" | long name "Instruction" | INTERNAL
        IFCSPACE "23" | long name "Service" | INTERNAL
        IFCSPACE "24" | long name "Service" | INTERNAL
        IFCSPACE "25" | long name "Service" | INTERNAL
      IFCBUILDINGSTOREY "Roof" | long name "Roof" | object type "Nivel:8mm Head" | elevation 11399.9999999999
        contains 29 elements
          1 x IFCROOF | object type "Cubierta básica:Concrete Deck - Tapered Insulation" | names: "Cubierta básica:Concrete Deck - Tapered Insulation:140056" | material: layers "Cubierta básica:Concrete Deck - Tapered Insulation" ("Roofing - EPDM Membrane" 2., "Insulation / Thermal Barriers - Rigid insulation" 50., "Concrete - Cast In Situ" 200.) | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | object type "Muro básico:Interior - 138mm Partition (1-hr)" | names: "Muro básico:Interior - 138mm Partition (1-hr):165698", "Muro básico:Interior - 138mm Partition (1-hr):165699", "Muro básico:Interior - 138mm Partition (1-hr):165700" (+9 more) | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Parapet Wall" | object type "Muro básico:Parapet Wall" | names: "Muro básico:Parapet Wall:167548", "Muro básico:Parapet Wall:167733", "Muro básico:Parapet Wall:167934" (+2 more) | material: layers "Muro básico:Parapet Wall" ("Insulation / Thermal Barriers - External Wall Insulation" 100., "Masonry - Concrete Block" 190.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Muro básico:Parapet Wall" | object type "Muro básico:Parapet Wall" | names: "Muro básico:Parapet Wall:168323", "Muro básico:Parapet Wall:168458", "Muro básico:Parapet Wall:168539" | material: layers "Muro básico:Parapet Wall" ("Insulation / Thermal Barriers - External Wall Insulation" 100., "Masonry - Concrete Block" 190.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192754" | names: "192754" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192755" | names: "192755" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192756" | names: "192756" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192757" | names: "192757" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192758" | names: "192758" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192759" | names: "192759" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192760" | names: "192760" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "192761" | names: "192761" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Parapet" | long name "Parapet" | object type "Nivel:8mm Head" | elevation 12000.
        contains 3 elements
          3 x IFCROOF | type IFCCURTAINWALLTYPE "Cristalera inclinada:Sloped Glazing" | object type "Cristalera inclinada:Sloped Glazing" | names: "Cristalera inclinada:Sloped Glazing:165755", "Cristalera inclinada:Sloped Glazing:167036", "Cristalera inclinada:Sloped Glazing:167158" | parts: 120 IFCMEMBER, 42 IFCPLATE | property sets: Pset_QuantityTakeOff, Pset_RoofCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Superficie:105545" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Subregión:111931" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Superficie:130736" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "M_Parking Space:5480 x 2740mm - 90 deg" | 27 occurrences | material: "Parking Stripe" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Scarlet Oak - 12.5 Meters" | 4 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Honey Locust - 7.6 Meters" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Shrub:Barberry - 1.0 Meters" | 11 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Red Maple - 9 Meters" | 3 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Golden Chain - 5.5 Meters" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Tree - Deciduous:Japanese Cherry - 4.5 Meters" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Shrub:Golden Flame Spirea - 0.8 Meters" | 6 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:Exterior - Insulation on Masonry" | STANDARD | 8 occurrences | material: layers "Muro básico:Exterior - Insulation on Masonry" ("Insulation / Thermal Barriers - External Wall Insulation" 100., "Masonry - Concrete Block" 190., "Plasterboard" 13.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCURTAINWALLTYPE "Muro cortina:Exterior Curtain Wall" | 18 occurrences | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
  IFCCURTAINWALLTYPE "Muro cortina:Pavillion Curtain Wall" | 3 occurrences | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 53 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Muro básico:Interior - 138mm Partition (1-hr)" | STANDARD | 122 occurrences | material: layers "Muro básico:Interior - 138mm Partition (1-hr)" ("Plasterboard" 15.5, "Metal - Stud Layer" 92., "Plasterboard" 15.5, "Plasterboard" 15.5) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Muro básico:Generic - 200mm" | STANDARD | 4 occurrences | material: layers "Muro básico:Generic - 200mm" ("Default Wall" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWINDOWSTYLE "M_Fixed:0915 x 1220mm" | 24 occurrences | material: materials ("Sash", "Sash", "Glass", "Sash") | property sets: M_Fixed:0915 x 1220mm:145607, Pset_QuantityTakeOff, Pset_WindowCommon
  IFCDOORSTYLE "M_Single-Flush-Dbl Acting:0915 x 2134mm" | DOUBLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush-Dbl Acting:0915 x 2134mm:145999, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | SINGLE_SWING_RIGHT | 31 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:146094, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm 20 Minute Rated:146152, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Flush:1830 x 2134mm" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Double-Flush:1830 x 2134mm:146282, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | SINGLE_SWING_LEFT | 30 occurrences | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush:0915 x 2134mm:146483, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush:0915 x 2134mm:146741, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Plain" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Plain" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCURTAINWALLTYPE "Muro cortina:Storefront" | 13 occurrences | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Double-Flush:1730 x 2134mm:149921, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Double-Flush:1730 x 2134mm 20 Minute Rated:150034, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Flush:1730 x 2134mm 20 Minute Rated" | DOUBLE_DOOR_SINGLE_SWING | 2 occurrences | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Double-Flush:1730 x 2134mm 20 Minute Rated:150153, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Flush:1830 x 2134mm" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Double-Flush:1830 x 2134mm:150584, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush:0915 x 2134mm:155278, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:Generic - 225mm Concrete" | STANDARD | 4 occurrences | material: layers "Muro básico:Generic - 225mm Concrete" ("Concrete - Cast-in-Place Concrete" 225.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Suelo:Standard Timber-Wood Finish" | FLOOR | 1 occurrence | material: layers "Suelo:Standard Timber-Wood Finish" ("Wood - Flooring" 40., "Concrete - Cast-in-Place Concrete" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_W-Wide Flange-Column:W250X49.1" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:450mm" | COLUMN | 6 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Suelo:Concrete- 100mm" | FLOOR | 1 occurrence | material: layers "Suelo:Concrete- 100mm" ("Concrete - Cast-in-Place Concrete" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Borde de losa:Slab Edge" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Borde de losa:Slab Edge" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCFURNITURETYPE "M_Table-Dining Round w Chairs:0915mm Diameter" | 15 occurrences | material: materials ("Wood - Pine", "Laminate - Linen, Matte") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "M_Chair-Breuer:M_Chair-Breuer" | 60 occurrences | material: materials ("Textile - Bamboo Weave", "Metal - Chrome") | property sets: Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Hollow Core Plank - Concrete Topping" | FLOOR | 1 occurrence | material: layers "Suelo:Hollow Core Plank - Concrete Topping" ("Carpet (1)" 15., "Concrete - Cast-in-Place Concrete" 50., "Concrete - Cast In Situ" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 54 occurrences | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "M_Single-Flush:0915 x 2134mm 20 Minute Rated" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm 20 Minute Rated:159676, Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "Pendant Light - Linear - 1 Lamp:2440mm - 277V" | 30 occurrences | material: materials ("Paint - Maroon Glossy", "Metal - Paint Finish - Ivory, Glossy", "Glass - White, High Luminance") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Hollow Core Plank - Concrete Topping" | FLOOR | 1 occurrence | material: layers "Suelo:Hollow Core Plank - Concrete Topping" ("Carpet (1)" 15., "Concrete - Cast-in-Place Concrete" 50., "Concrete - Cast In Situ" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "M_Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "M_Single-Flush Vision:0915 x 2134mm" | 2 occurrences | material: materials ("Door - Panel", "Paint - Maroon Glossy") | property sets: M_Single-Flush Vision:0915 x 2134mm:164566, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Flush Vision:0915 x 2134mm" | 2 occurrences | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: M_Single-Flush Vision:0915 x 2134mm:164626, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Double-Glass 1:1830 x 2134mm" | 1 occurrence | material: materials ("Paint - Maroon Glossy", "Door - Panel") | property sets: M_Double-Glass 1:1830 x 2134mm:165368, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "M_Single-Glass 1:0915 x 2134mm" | 1 occurrence | material: materials ("Door - Panel", "Paint - Maroon Glossy") | property sets: M_Single-Glass 1:0915 x 2134mm:165525, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:600 x 600mm Grid" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Metal Sunscreen" | FLOOR | 1 occurrence | material: layers "Suelo:Metal Sunscreen" ("Metal - Sunscreen" 12.7) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Techo compuesto:Furred Ceiling" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCFURNITURETYPE "Chair-Viper:Chair" | 7 occurrences | material: "Leather - Brown, Pebble" | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Couch-Viper:Couch" | 3 occurrences | material: "Leather - Tan" | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Wastebasket2:Wastebasket2" | 4 occurrences | material: "Plastic - Dark Maroon, Smooth" | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Table-Night Stand:24" x 24" x 30"" | 9 occurrences | material: materials ("Wood - Cherry", "Wood - Cherry") | property sets: Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Potted Plant:Potted Plant" | 2 occurrences | material: "Ceramic - Tan" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "Table Lamp 4:60 watt Incandescent" | 4 occurrences | material: materials ("Metal - Bronze", "Shade - Beige, texture") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "Sconce 4:40 watt Halogen" | 7 occurrences | material: materials ("Glass - Clear Light", "Metal - Chrome", "Default Light Source") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Wood - Birch", "Fabric - Mesh") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Fabric - Mesh", "Wood - Birch") | property sets: Pset_QuantityTakeOff
  IFCFURNITURETYPE "Window Shade:Window Shade" | 1 occurrence | material: materials ("Wood - Birch", "Fabric - Mesh") | property sets: Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Male:Alex" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Male:Jay" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_RPC Female:Florence" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:Parapet Wall" | STANDARD | 8 occurrences | material: layers "Muro básico:Parapet Wall" ("Insulation / Thermal Barriers - External Wall Insulation" 100., "Masonry - Concrete Block" 190.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "192754" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192755" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192756" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192757" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192758" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192759" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192760" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "192761" | 1 occurrence
  IFCCURTAINWALLTYPE "Cristalera inclinada:Sloped Glazing" | 3 occurrences | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff

Property sets
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Vest. 101" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Lobby 102" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Conference 103" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Instruction 104" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Instruction 105" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Instruction 106" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Corridor 107" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Instruction 108" (IFCIDENTIFIER)
  Pset_SpaceCommon: 108 more contents on 108 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 27 objects (27 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "5480 x 2740mm - 90 deg" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Barberry - 1.0 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Reference = "" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Golden Flame Spirea - 0.8 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Scarlet Oak - 12.5 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Red Maple - 9 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Slab Edge" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Honey Locust - 7.6 Meters" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 6 more contents on 9 objects not shown
  Pset_QuantityTakeOff | properties | on 3077 objects (3077 IFCMEMBER)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1190 objects (1190 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 164 objects (164 IFCCOLUMN) | on 59 type objects
    Reference = "300mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 159 objects (159 IFCPLATE)
    Reference = "Solid" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 123 objects (119 IFCWALLSTANDARDCASE, 3 IFCWALL, 1 IFCOPENINGELEMENT) | on 1 type object
    Reference = "Interior - 138mm Partition (1-hr)" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 120 objects (120 IFCMEMBER)
    Reference = "30mm Square" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 79 objects (79 IFCMEMBER)
    Reference = "L Mullion 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 72 objects (32 IFCMEMBER, 20 IFCSTAIRFLIGHT, 10 IFCSLAB, 10 IFCSTAIR)
    Reference = "150mm max riser 300mm tread" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 56 more contents on 563 objects not shown
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 3.175 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 101.600000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 3.175 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ReinforcementBarPitchOfSlab | properties | on 12 objects (12 IFCSLAB) | on 12 type objects
    Reference = "Metal Sunscreen" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 10 objects (10 IFCSLAB)
    Reference = "150mm max riser 300mm tread" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Hollow Core Plank - Concrete Topping" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Generic - 400mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Standard Timber-Wood Finish" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Concrete- 100mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Generic - 75mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 12 objects (12 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Metal Sunscreen" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 10 objects (10 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "150mm max riser 300mm tread" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Hollow Core Plank - Concrete Topping" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 15. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Standard Timber-Wood Finish" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 1.74230016614259 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic - 75mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concrete- 100mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 12 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Metal Sunscreen" (IFCIDENTIFIER)
  Pset_SlabCommon: 3 more contents on 0 objects not shown
  Pset_OpeningElementCommon | properties | on 14 objects (14 IFCOPENINGELEMENT)
    Reference = "Hollow Core Plank - Concrete Topping" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 8 objects (8 IFCOPENINGELEMENT)
    Reference = "Reveal" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 5 objects (3 IFCOPENINGELEMENT, 2 IFCCURTAINWALL)
    Reference = "Exterior Curtain Wall" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Exterior - Insulation on Masonry" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Interior - 138mm Partition (1-hr)" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 122 objects (119 IFCWALLSTANDARDCASE, 3 IFCWALL) | on 1 type object
    Reference = "Interior - 138mm Partition (1-hr)" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 9 objects (8 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT) | on 1 type object
    Reference = "Exterior - Insulation on Masonry" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (5 IFCWALLSTANDARDCASE, 3 IFCWALL) | on 1 type object
    Reference = "Parapet Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Generic - 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Generic - 225mm Concrete" (IFCLABEL)
  Pset_WallCommon | properties | on 102 objects (99 IFCWALLSTANDARDCASE, 3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 138mm Partition (1-hr)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 138mm Partition (1-hr)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 9 objects (8 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Exterior - Insulation on Masonry" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (5 IFCWALLSTANDARDCASE, 3 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Parapet Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 225mm Concrete" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Exterior - Insulation on Masonry" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Interior - 138mm Partition (1-hr)" (IFCIDENTIFIER)
  Pset_WallCommon: 3 more contents on 0 objects not shown
  Pset_CurtainWallCommon | properties | on 16 objects (16 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Exterior Curtain Wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 13 objects (13 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Storefront" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Pavillion Curtain Wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Exterior Curtain Wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pavillion Curtain Wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Storefront" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Sloped Glazing" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 1190 objects (1190 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 159 objects (159 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Solid" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 924 objects (924 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1265. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 856 objects (856 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1950. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 122 objects (122 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 610. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 118 objects (118 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 1290. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 88 objects (88 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 2000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 61 objects (61 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 2390. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 56 objects (56 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 2159. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 48 objects (48 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "L Mullion 1" (IFCIDENTIFIER)
    Span = 1265. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 146 more contents on 1035 objects not shown
  Pset_DoorCommon | properties | on 69 objects (69 IFCDOOR) | on 8 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 11 objects (11 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "M_Curtain Wall Sgl Glass" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR) | on 2 type objects
    FireRating = "20 Minute" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm 20 Minute Rated" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "M_Curtain Wall Dbl Glass" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR) | on 2 type objects
    FireRating = "20 Minute" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1730 x 2134mm 20 Minute Rated" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR) | on 3 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1830 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1730 x 2134mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Concrete Deck - Tapered Insulation" (IFCIDENTIFIER)
    TotalArea = 1592.5849489241 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 53.703242949303 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
    TotalArea = 55.5976882361891 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 25.0533069600242 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Sloped Glazing" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 25.1483591600241 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Sloped Glazing" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 25.4026149600243 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Sloped Glazing" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 71.0637766976648 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Generic - 75mm" (IFCIDENTIFIER)
    TotalArea = 71.0939797905742 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_ColumnCommon | properties | on 164 objects (164 IFCCOLUMN) | on 59 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "300mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN) | on 6 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W250X49.1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "450mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 164 objects (164 IFCCOLUMN) | on 59 type objects
    Reference = "300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 6 objects (6 IFCCOLUMN) | on 6 type objects
    Reference = "W250X49.1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 6 objects (6 IFCCOLUMN) | on 1 type object
    Reference = "450mm" (IFCLABEL)
  Pset_WindowCommon | properties | on 24 objects (24 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 1220mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 1220mm" (IFCIDENTIFIER)
  Pset_ConcreteElementGeneral | properties | on 10 objects (10 IFCDOOR) | on 4 type objects
    FireRating = "20 Minute" (IFCLABEL)
  Pset_CoveringCommon | properties | on 60 objects (60 IFCCOVERING)
    Finish = "Ceiling Tile 600 x 600;" (IFCTEXT)
    Reference = "600 x 600mm Grid" (IFCIDENTIFIER)
    TotalThickness = 52. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    Finish = "Plasterboard;" (IFCTEXT)
    Reference = "Furred Ceiling" (IFCIDENTIFIER)
    TotalThickness = 38.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    Reference = "Plain" (IFCIDENTIFIER)
    TotalThickness = 57. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 60 type objects
    Reference = "600 x 600mm Grid" (IFCIDENTIFIER)
    TotalThickness = 52. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 3 type objects
    Reference = "Furred Ceiling" (IFCIDENTIFIER)
    TotalThickness = 38.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 5 (IFCINTEGER)
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_StairFlightCommon | properties | on 12 objects (12 IFCSTAIRFLIGHT)
    NosingLength = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 25. (IFCCOUNTMEASURE)
    NumberOfTreads = 25. (IFCCOUNTMEASURE)
    Reference = "150mm max riser 300mm tread" (IFCIDENTIFIER)
    RiserHeight = 146.153846153903 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 570. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 8 objects (8 IFCSTAIRFLIGHT)
    NosingLength = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 25. (IFCCOUNTMEASURE)
    NumberOfTreads = 25. (IFCCOUNTMEASURE)
    Reference = "150mm max riser 300mm tread" (IFCIDENTIFIER)
    RiserHeight = 146.153846153903 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 812.5 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 10 objects (10 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 25. (IFCCOUNTMEASURE)
    NumberOfTreads = 25. (IFCCOUNTMEASURE)
    Reference = "150mm max riser 300mm tread" (IFCIDENTIFIER)
    RiserHeight = 146.153846153903 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RailingCommon | properties | on 14 objects (14 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "900mm Pipe" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 12 objects (12 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "900mm Pipe - Wall Monted" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 9 objects (9 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Guardrail - Pipe" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 30 objects (30 IFCFLOWTERMINAL) | on 1 type object
    Reference = "2440mm - 277V" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 7 objects (7 IFCFLOWTERMINAL) | on 1 type object
    Reference = "40 watt Halogen" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 4 objects (4 IFCFLOWTERMINAL) | on 1 type object
    Reference = "60 watt Incandescent" (IFCIDENTIFIER)
  M_Fixed:0915 x 1220mm:145607 | predefined | on 1 type object
  M_Single-Flush-Dbl Acting:0915 x 2134mm:145999 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:146094 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm 20 Minute Rated:146152 | predefined | on 2 type objects
  M_Double-Flush:1830 x 2134mm:146282 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:146483 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:146741 | predefined | on 2 type objects
  M_Double-Flush:1730 x 2134mm:149921 | predefined | on 2 type objects
  M_Double-Flush:1730 x 2134mm 20 Minute Rated:150034 | predefined | on 2 type objects
  M_Double-Flush:1730 x 2134mm 20 Minute Rated:150153 | predefined | on 2 type objects
  M_Double-Flush:1830 x 2134mm:150584 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm:155278 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2134mm 20 Minute Rated:159676 | predefined | on 2 type objects
  M_Single-Flush Vision:0915 x 2134mm:164566 | predefined | on 2 type objects
  M_Single-Flush Vision:0915 x 2134mm:164626 | predefined | on 2 type objects
  M_Double-Glass 1:1830 x 2134mm:165368 | predefined | on 2 type objects
  M_Single-Glass 1:0915 x 2134mm:165525 | predefined | on 2 type objects